Thermal Pad Dimensions
RTX 2080 SEA HAWK EK X
[image: Diagram

Description automatically generated]

[image: Diagram

Description automatically generated][image: ]
[image: Diagram, engineering drawing

Description automatically generated]

[image: Diagram

Description automatically generated with medium confidence]
[image: Diagram, engineering drawing

Description automatically generated]

image4.jpeg
Ak

15£3 24.5%0.5

(a3

S|
il
Y

3+0.3

s —r




image5.jpeg
15£3

5608

FIEYS

1240.5,

Bt R

303





image6.jpeg
Fa£7e

10+3

S5%0.5

FEHRARIE

2.5+0.25





image1.jpeg
TP SH 0,5mm (30x16mm)

TP SH 1mim (10x10mm) T8 $H 0 5mm (60xt6mm)

T $H 0 smm (30<6mm)

TP SH 1mm (20x10mm) TP SH 1mm (1636mm)

TP SH 1mm (105x16mm) T8 5H 1mim (6x6mim)




image2.jpeg




image3.jpeg
15 36305

ik

36405

30,

e ——




